<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.1">
<drawing>
<board>
<plain>
<text>C0000</text>
<text>C4000</text>
<text>C8000</text>
<text>CC000</text>
<text>OFF</text>
<text>OFF</text>
<text>ON</text>
<text>ON</text>
<text>OFF</text>
<text>OFF</text>
<text>ON</text>
<text>ON</text>
<text>2</text>
<text>3</text>
<text>Rev.A</text>
<text>JR-IDE/ISA</text>
<text>ALH</text>
<text>retrotronics.org/jride_isa</text>
<text>D0000</text>
<text>D4000</text>
<text>D8000</text>
<text>DC000</text>
<text>OFF</text>
<text>OFF</text>
<text>ON</text>
<text>ON</text>
<text>OFF</text>
<text>OFF</text>
<text>ON</text>
<text>ON</text>
<text>OFF</text>
<text>OFF</text>
<text>OFF</text>
<text>OFF</text>
<text>1</text>
<text>ON</text>
<text>ON</text>
<text>ON</text>
<text>ON</text>
<text>ByteBlaster/II/MV</text>
<text>GND</text>
<text>+5V</text>
<text>N.C.</text>
<text>N.C.</text>
<text>GND</text>
<text>TCK</text>
<text>TDO</text>
<text>TMS</text>
<text>N.C.</text>
<text>TDI</text>
<text>Aux. Power Out</text>
<text>ON</text>
<text>A</text>
<text>K</text>
<text>IDE Key-Pin 20</text>
<text>+5V Enable</text>
<text>HD LED</text>
<text>16 KB Option ROM:</text>
<text>SW1-4 = Enable</text>
<text>+5V</text>
<text>GND</text>
<text>GND</text>
<text>+5V</text>
</plain>
<libraries>
<library name="alan_common">
<packages>
<package name="OSHW_LOGO">
</package>
<package name="ISA_XTIDE_MK25">
</package>
<package name="PLCC84">
</package>
<package name="HDR_1X2">
</package>
<package name="HDR_2X20">
</package>
<package name="C_TH_5MM">
<description>CAPACITOR
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="R_204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="HDR_2X5">
</package>
<package name="HDR_1X4">
</package>
<package name="LED_TH_3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="DIL32W_ROUND">
</package>
<package name="SW_DIP-4_ROUND">
</package>
<package name="RN_SIP5">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C5" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="alan_common" package="PLCC84" value="ATF1508AS[L]">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HDLED" library="alan_common" package="LED_TH_3MM" value="">
<attribute name="VALUE"/>
</element>
<element name="R2" library="alan_common" package="R_204/7" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="alan_common" package="HDR_1X2" value="HDR_1X2"/>
<element name="U$1" library="alan_common" package="OSHW_LOGO" value="OSHW_LOGO"/>
<element name="C7" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="alan_common" package="C_TH_5MM" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CONN1" library="alan_common" package="ISA_XTIDE_MK25" value="8-BIT ISA CARD EDGE"/>
<element name="J1" library="alan_common" package="HDR_2X20" value="PATA_HD">
<attribute name="NAME"/>
</element>
<element name="U2" library="alan_common" package="DIL32W_ROUND" value="SST39SF0x0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JTAG-ISP" library="alan_common" package="HDR_2X5" value="HDR_2X5&quot;">
<attribute name="NAME"/>
</element>
<element name="J2" library="alan_common" package="HDR_1X4" value="HDR_1X4">
<attribute name="NAME"/>
</element>
<element name="C2" library="alan_common" package="C_TH_5MM" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="alan_common" package="R_204/7" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="alan_common" package="HDR_1X2" value="HDR_1X2">
<attribute name="NAME"/>
</element>
<element name="R1" library="alan_common" package="R_204/7" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="alan_common" package="SW_DIP-4_ROUND" value="SW_DIP-4R">
<attribute name="NAME"/>
</element>
<element name="RN1" library="alan_common" package="RN_SIP5" value="10K">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="D1">
<contactref element="CONN1" pad="A8"/>
<contactref element="U1" pad="70"/>
</signal>
<signal name="D2">
<contactref element="CONN1" pad="A7"/>
<contactref element="U1" pad="73"/>
</signal>
<signal name="D4">
<contactref element="CONN1" pad="A5"/>
<contactref element="U1" pad="76"/>
</signal>
<signal name="D7">
<contactref element="CONN1" pad="A2"/>
<contactref element="U1" pad="80"/>
</signal>
<signal name="A0">
<contactref element="CONN1" pad="A31"/>
<contactref element="U2" pad="12"/>
<contactref element="U1" pad="35"/>
</signal>
<signal name="A2">
<contactref element="CONN1" pad="A29"/>
<contactref element="U2" pad="10"/>
<contactref element="U1" pad="40"/>
</signal>
<signal name="A5">
<contactref element="CONN1" pad="A26"/>
<contactref element="U2" pad="7"/>
<contactref element="U1" pad="44"/>
</signal>
<signal name="A6">
<contactref element="CONN1" pad="A25"/>
<contactref element="U2" pad="6"/>
<contactref element="U1" pad="45"/>
</signal>
<signal name="A8">
<contactref element="CONN1" pad="A23"/>
<contactref element="U2" pad="27"/>
<contactref element="U1" pad="51"/>
</signal>
<signal name="A11">
<contactref element="CONN1" pad="A20"/>
<contactref element="U1" pad="56"/>
<contactref element="U2" pad="25"/>
</signal>
<signal name="A12">
<contactref element="CONN1" pad="A19"/>
<contactref element="U2" pad="4"/>
<contactref element="U1" pad="57"/>
</signal>
<signal name="A15">
<contactref element="CONN1" pad="A16"/>
<contactref element="U1" pad="60"/>
</signal>
<signal name="A17">
<contactref element="CONN1" pad="A14"/>
<contactref element="U1" pad="63"/>
</signal>
<signal name="A19">
<contactref element="CONN1" pad="A12"/>
<contactref element="U1" pad="65"/>
</signal>
<signal name="!MEMR">
<contactref element="CONN1" pad="B12"/>
<contactref element="U1" pad="67"/>
</signal>
<signal name="!MEMW">
<contactref element="CONN1" pad="B11"/>
<contactref element="U1" pad="68"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="1"/>
<contactref element="CONN1" pad="B2"/>
</signal>
<signal name="A18">
<contactref element="CONN1" pad="A13"/>
<contactref element="U1" pad="64"/>
</signal>
<signal name="A16">
<contactref element="CONN1" pad="A15"/>
<contactref element="U1" pad="61"/>
</signal>
<signal name="A14">
<contactref element="CONN1" pad="A17"/>
<contactref element="U1" pad="52"/>
</signal>
<signal name="A13">
<contactref element="CONN1" pad="A18"/>
<contactref element="U1" pad="58"/>
</signal>
<signal name="A10">
<contactref element="CONN1" pad="A21"/>
<contactref element="U2" pad="23"/>
<contactref element="U1" pad="54"/>
</signal>
<signal name="A9">
<contactref element="CONN1" pad="A22"/>
<contactref element="U2" pad="26"/>
<contactref element="U1" pad="55"/>
</signal>
<signal name="A7">
<contactref element="CONN1" pad="A24"/>
<contactref element="U2" pad="5"/>
<contactref element="U1" pad="46"/>
</signal>
<signal name="A4">
<contactref element="CONN1" pad="A27"/>
<contactref element="U2" pad="8"/>
<contactref element="U1" pad="41"/>
</signal>
<signal name="A3">
<contactref element="CONN1" pad="A28"/>
<contactref element="U2" pad="9"/>
<contactref element="U1" pad="39"/>
</signal>
<signal name="A1">
<contactref element="CONN1" pad="A30"/>
<contactref element="U2" pad="11"/>
<contactref element="U1" pad="36"/>
</signal>
<signal name="D6">
<contactref element="CONN1" pad="A3"/>
<contactref element="U1" pad="77"/>
</signal>
<signal name="D5">
<contactref element="CONN1" pad="A4"/>
<contactref element="U1" pad="75"/>
</signal>
<signal name="D3">
<contactref element="CONN1" pad="A6"/>
<contactref element="U1" pad="74"/>
</signal>
<signal name="D0">
<contactref element="CONN1" pad="A9"/>
<contactref element="U1" pad="69"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="72"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="19"/>
<contactref element="U1" pad="82"/>
<contactref element="U1" pad="59"/>
<contactref element="U1" pad="47"/>
<contactref element="U1" pad="32"/>
<contactref element="U1" pad="42"/>
<contactref element="C5" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="CONN1" pad="B1"/>
<contactref element="J1" pad="19"/>
<contactref element="J1" pad="40"/>
<contactref element="J1" pad="30"/>
<contactref element="J1" pad="26"/>
<contactref element="J1" pad="24"/>
<contactref element="J1" pad="22"/>
<contactref element="J1" pad="2"/>
<contactref element="U2" pad="16"/>
<contactref element="JTAG-ISP" pad="10"/>
<contactref element="JTAG-ISP" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="J2" pad="3"/>
<contactref element="C2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="J1" pad="28"/>
<contactref element="SW1" pad="6"/>
<contactref element="SW1" pad="7"/>
<contactref element="SW1" pad="8"/>
<contactref element="SW1" pad="5"/>
<contactref element="CONN1" pad="B10"/>
<contactref element="CONN1" pad="B31"/>
<contactref element="CONN1" pad="S1"/>
<contactref element="CONN1" pad="S2"/>
</signal>
<signal name="+5V">
<contactref element="C5" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="38"/>
<contactref element="U1" pad="26"/>
<contactref element="U1" pad="13"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="78"/>
<contactref element="U1" pad="66"/>
<contactref element="U1" pad="43"/>
<contactref element="U1" pad="53"/>
<contactref element="C4" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="CONN1" pad="B3"/>
<contactref element="U2" pad="32"/>
<contactref element="JTAG-ISP" pad="4"/>
<contactref element="J2" pad="1"/>
<contactref element="J2" pad="4"/>
<contactref element="C2" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="RN1" pad="1"/>
<contactref element="CONN1" pad="B29"/>
</signal>
<signal name="IDE_D15">
<contactref element="J1" pad="18"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="IDE_D7">
<contactref element="J1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="U2" pad="21"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="IDE_D6">
<contactref element="J1" pad="5"/>
<contactref element="U1" pad="8"/>
<contactref element="U2" pad="20"/>
</signal>
<signal name="IDE_D5">
<contactref element="J1" pad="7"/>
<contactref element="U1" pad="11"/>
<contactref element="U2" pad="19"/>
</signal>
<signal name="IDE_D4">
<contactref element="J1" pad="9"/>
<contactref element="U1" pad="12"/>
<contactref element="U2" pad="18"/>
</signal>
<signal name="IDE_D3">
<contactref element="J1" pad="11"/>
<contactref element="U1" pad="16"/>
<contactref element="U2" pad="17"/>
</signal>
<signal name="IDE_D2">
<contactref element="J1" pad="13"/>
<contactref element="U1" pad="21"/>
<contactref element="U2" pad="15"/>
</signal>
<signal name="IDE_D1">
<contactref element="J1" pad="15"/>
<contactref element="U1" pad="22"/>
<contactref element="U2" pad="14"/>
</signal>
<signal name="IDE_D0">
<contactref element="J1" pad="17"/>
<contactref element="U1" pad="24"/>
<contactref element="U2" pad="13"/>
</signal>
<signal name="CFG2">
<contactref element="U1" pad="84"/>
<contactref element="SW1" pad="2"/>
<contactref element="RN1" pad="4"/>
</signal>
<signal name="CFG3">
<contactref element="U1" pad="83"/>
<contactref element="SW1" pad="3"/>
<contactref element="RN1" pad="3"/>
</signal>
<signal name="CFG1">
<contactref element="U1" pad="2"/>
<contactref element="SW1" pad="1"/>
<contactref element="RN1" pad="5"/>
</signal>
<signal name="!DASP">
<contactref element="HDLED" pad="K"/>
<contactref element="J1" pad="39"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="HDLED" pad="A"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="!ROM_CS">
<contactref element="U2" pad="22"/>
<contactref element="U1" pad="37"/>
</signal>
<signal name="TMS">
<contactref element="U1" pad="23"/>
<contactref element="JTAG-ISP" pad="5"/>
</signal>
<signal name="TDI">
<contactref element="U1" pad="14"/>
<contactref element="JTAG-ISP" pad="9"/>
</signal>
<signal name="TDO">
<contactref element="U1" pad="71"/>
<contactref element="JTAG-ISP" pad="3"/>
</signal>
<signal name="TCK">
<contactref element="U1" pad="62"/>
<contactref element="JTAG-ISP" pad="1"/>
</signal>
<signal name="!IDE_IOW">
<contactref element="J1" pad="23"/>
<contactref element="U1" pad="27"/>
<contactref element="U2" pad="31"/>
</signal>
<signal name="!IDE_IOR">
<contactref element="J1" pad="25"/>
<contactref element="U1" pad="28"/>
<contactref element="U2" pad="24"/>
</signal>
<signal name="IDE_A1">
<contactref element="J1" pad="33"/>
<contactref element="U1" pad="29"/>
<contactref element="U2" pad="30"/>
</signal>
<signal name="IDE_A0">
<contactref element="J1" pad="35"/>
<contactref element="U1" pad="30"/>
<contactref element="U2" pad="28"/>
</signal>
<signal name="!IDE_CS0">
<contactref element="J1" pad="37"/>
<contactref element="U1" pad="34"/>
</signal>
<signal name="IDE_D8">
<contactref element="J1" pad="4"/>
<contactref element="U1" pad="6"/>
</signal>
<signal name="IDE_D9">
<contactref element="J1" pad="6"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="IDE_D10">
<contactref element="J1" pad="8"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="IDE_D11">
<contactref element="J1" pad="10"/>
<contactref element="U1" pad="15"/>
</signal>
<signal name="IDE_D12">
<contactref element="J1" pad="12"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="IDE_D13">
<contactref element="J1" pad="14"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="IDE_D14">
<contactref element="J1" pad="16"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="IDE_A2">
<contactref element="J1" pad="36"/>
<contactref element="U1" pad="31"/>
<contactref element="U2" pad="29"/>
</signal>
<signal name="!RESET">
<contactref element="J1" pad="1"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="!IDE_CS1">
<contactref element="J1" pad="38"/>
<contactref element="U1" pad="33"/>
</signal>
<signal name="ROM_A15">
<contactref element="U2" pad="3"/>
<contactref element="U1" pad="48"/>
</signal>
<signal name="ROM_A16">
<contactref element="U2" pad="2"/>
<contactref element="U1" pad="49"/>
</signal>
<signal name="ROM_A18">
<contactref element="U2" pad="1"/>
<contactref element="U1" pad="50"/>
</signal>
<signal name="CLK">
<contactref element="CONN1" pad="B20"/>
<contactref element="U1" pad="81"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="20"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="J4" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="CFG4">
<contactref element="SW1" pad="4"/>
<contactref element="RN1" pad="2"/>
<contactref element="U1" pad="79"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
