<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<text>C0000</text>
<text>C4000</text>
<text>C8000</text>
<text>CC000</text>
<text>OFF</text>
<text>OFF</text>
<text>ON</text>
<text>ON</text>
<text>OFF</text>
<text>OFF</text>
<text>ON</text>
<text>ON</text>
<text>4</text>
<text>5</text>
<text>ROM</text>
<text>IRQ1</text>
<text>IRQ2</text>
<text>IRQ7</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>ON</text>
<text>OFF</text>
<text>OFF</text>
<text>OFF</text>
<text>OFF</text>
<text>ON</text>
<text>OFF</text>
<text>OFF</text>
<text>ON</text>
<text>----</text>
<text>OFF</text>
<text>OFF</text>
<text>OFF</text>
<text>RTC</text>
<text>Rev.B</text>
<text>JTAG - ISP</text>
<text>JR-IDE</text>
<text>ALH</text>
<text>JTAG - ISP</text>
<text>retrotronics.org/jride</text>
<text>+5V</text>
<text>GND</text>
<text>SW1-6: ROM Enable</text>
<text>+5V on Pin 20</text>
<wire x1="0" y1="0" x2="-25.4" y2="0" width="0.127" layer="20"/>
<wire x1="-25.4" y1="0" x2="-25.4" y2="48.26" width="0.127" layer="20"/>
<wire x1="-25.4" y1="48.26" x2="2.54" y2="76.2" width="0.127" layer="20"/>
<wire x1="2.54" y1="76.2" x2="171.45" y2="76.2" width="0.127" layer="20"/>
<wire x1="171.45" y1="76.2" x2="171.45" y2="0" width="0.127" layer="20"/>
<text>CR2032</text>
<text>+BAT</text>
<text>GND</text>
</plain>
<libraries>
<library name="alan_common">
<packages>
<package name="7SEG_2X">
</package>
<package name="PLCC44">
</package>
<package name="DIL16">
</package>
<package name="SW_DIP-6">
</package>
<package name="PCJR_SIDECAR_SHORT">
</package>
<package name="C_TH_5MM">
<description>CAPACITOR
grid 5 mm, outline 2.5 x 7.5 mm</description>
</package>
<package name="PLCC84">
</package>
<package name="R_204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="HDR_1X2">
</package>
<package name="HDR_2X5">
</package>
<package name="DIL32W">
</package>
<package name="LED_TH_3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="RN_SIP4">
</package>
<package name="HDR_2X20">
</package>
<package name="BAT_PTH_CR2032">
</package>
<package name="DIL24W">
</package>
</packages>
</library>
<library name="logo">
<packages>
<package name="TONNE_10.00">
<description>&lt;b&gt;Logo trash / Mülltone 10 mm&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BUS" library="alan_common" package="PCJR_SIDECAR_SHORT" value="PCJR_SIDECAR_SHORT"/>
<element name="U2" library="alan_common" package="DIL32W" value="AS6C4008">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C1" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="U1" library="alan_common" package="DIL32W" value="AS6C4008">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="alan_common" package="PLCC84" value="ATF1508AS">
<attribute name="NAME"/>
</element>
<element name="C3" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C7" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="U3" library="alan_common" package="DIL32W" value="SST39SF040A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="POST" library="alan_common" package="7SEG_2X" value="LTD-4708JR"/>
<element name="HDLED" library="alan_common" package="LED_TH_3MM" value="LED">
<attribute name="NAME"/>
</element>
<element name="R1" library="alan_common" package="R_204/7" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="alan_common" package="HDR_1X2" value="HDR_1X2"/>
<element name="U6" library="alan_common" package="PLCC44" value="ATF1504AS">
<attribute name="NAME"/>
</element>
<element name="C5" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="RA1" library="alan_common" package="DIL16" value="220">
<attribute name="NAME"/>
</element>
<element name="U$5" library="logo" package="TONNE_10.00" value=""/>
<element name="C4" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="C9" library="alan_common" package="C_TH_5MM" value="22uF">
<attribute name="NAME"/>
</element>
<element name="J2" library="alan_common" package="HDR_2X20" value="PATA_HD">
<attribute name="NAME"/>
</element>
<element name="J3" library="alan_common" package="HDR_2X5" value="HDR_2X5&quot;"/>
<element name="J4" library="alan_common" package="HDR_2X5" value="HDR_2X5&quot;"/>
<element name="SW1" library="alan_common" package="SW_DIP-6" value="SW_DIP-6">
<attribute name="NAME"/>
</element>
<element name="RN1" library="alan_common" package="RN_SIP4" value="10K">
<attribute name="NAME"/>
</element>
<element name="R3" library="alan_common" package="R_204/7" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="alan_common" package="C_TH_5MM" value=".1uF">
<attribute name="NAME"/>
</element>
<element name="R2" library="alan_common" package="R_204/7" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="alan_common" package="HDR_1X2" value="HDR_1X2">
<attribute name="NAME"/>
</element>
<element name="AUX" library="alan_common" package="HDR_1X2" value="HDR_1X2">
<attribute name="NAME"/>
</element>
<element name="C11" library="alan_common" package="C_TH_5MM" value="22uF">
<attribute name="NAME"/>
</element>
<element name="VBAT" library="alan_common" package="BAT_PTH_CR2032" value="CR2032"/>
<element name="U5" library="alan_common" package="DIL24W" value="DS12885/7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BAT" library="alan_common" package="HDR_1X2" value="HDR_1X2"/>
<element name="C12" library="alan_common" package="C_TH_5MM" value="22uF">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="D1">
<contactref element="BUS" pad="B1"/>
<contactref element="U3" pad="14"/>
<contactref element="U2" pad="14"/>
<contactref element="U1" pad="14"/>
<contactref element="U6" pad="16"/>
<contactref element="U4" pad="49"/>
<contactref element="U5" pad="5"/>
</signal>
<signal name="D2">
<contactref element="BUS" pad="B2"/>
<contactref element="U3" pad="15"/>
<contactref element="U2" pad="15"/>
<contactref element="U1" pad="15"/>
<contactref element="U6" pad="17"/>
<contactref element="U4" pad="50"/>
<contactref element="U5" pad="6"/>
</signal>
<signal name="D4">
<contactref element="BUS" pad="B3"/>
<contactref element="U3" pad="18"/>
<contactref element="U2" pad="18"/>
<contactref element="U1" pad="18"/>
<contactref element="U6" pad="6"/>
<contactref element="U4" pad="54"/>
<contactref element="U5" pad="8"/>
</signal>
<signal name="D7">
<contactref element="BUS" pad="B5"/>
<contactref element="U3" pad="21"/>
<contactref element="U2" pad="21"/>
<contactref element="U1" pad="21"/>
<contactref element="U6" pad="9"/>
<contactref element="U4" pad="57"/>
<contactref element="U5" pad="11"/>
</signal>
<signal name="A0">
<contactref element="BUS" pad="B6"/>
<contactref element="U3" pad="12"/>
<contactref element="U1" pad="12"/>
<contactref element="U2" pad="12"/>
<contactref element="U6" pad="11"/>
<contactref element="U4" pad="74"/>
</signal>
<signal name="A2">
<contactref element="BUS" pad="B7"/>
<contactref element="U2" pad="10"/>
<contactref element="U1" pad="10"/>
<contactref element="U3" pad="10"/>
<contactref element="U4" pad="70"/>
</signal>
<signal name="A5">
<contactref element="BUS" pad="B9"/>
<contactref element="U2" pad="7"/>
<contactref element="U1" pad="7"/>
<contactref element="U3" pad="7"/>
<contactref element="U4" pad="67"/>
</signal>
<signal name="A6">
<contactref element="BUS" pad="B10"/>
<contactref element="U2" pad="6"/>
<contactref element="U1" pad="6"/>
<contactref element="U3" pad="6"/>
<contactref element="U4" pad="64"/>
<contactref element="U6" pad="19"/>
</signal>
<signal name="A8">
<contactref element="BUS" pad="B11"/>
<contactref element="U2" pad="27"/>
<contactref element="U1" pad="27"/>
<contactref element="U3" pad="27"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="A11">
<contactref element="BUS" pad="B13"/>
<contactref element="U2" pad="25"/>
<contactref element="U1" pad="25"/>
<contactref element="U3" pad="25"/>
<contactref element="U4" pad="81"/>
</signal>
<signal name="A12">
<contactref element="BUS" pad="B14"/>
<contactref element="U2" pad="4"/>
<contactref element="U1" pad="4"/>
<contactref element="U3" pad="4"/>
<contactref element="U4" pad="63"/>
</signal>
<signal name="A15">
<contactref element="BUS" pad="B16"/>
<contactref element="U2" pad="31"/>
<contactref element="U1" pad="31"/>
<contactref element="U4" pad="60"/>
</signal>
<signal name="A17">
<contactref element="BUS" pad="B18"/>
<contactref element="U2" pad="30"/>
<contactref element="U1" pad="30"/>
<contactref element="U4" pad="61"/>
</signal>
<signal name="A19">
<contactref element="BUS" pad="B19"/>
<contactref element="U4" pad="75"/>
</signal>
<signal name="!MEMR">
<contactref element="BUS" pad="B21"/>
<contactref element="U2" pad="24"/>
<contactref element="U1" pad="24"/>
<contactref element="U3" pad="24"/>
<contactref element="U4" pad="80"/>
</signal>
<signal name="!MEMW">
<contactref element="BUS" pad="B22"/>
<contactref element="U2" pad="29"/>
<contactref element="U1" pad="29"/>
<contactref element="U3" pad="31"/>
<contactref element="U4" pad="79"/>
</signal>
<signal name="RESET">
<contactref element="BUS" pad="A25"/>
<contactref element="U4" pad="1"/>
<contactref element="U6" pad="1"/>
</signal>
<signal name="A18">
<contactref element="BUS" pad="A19"/>
<contactref element="U2" pad="1"/>
<contactref element="U1" pad="1"/>
<contactref element="U4" pad="46"/>
</signal>
<signal name="A16">
<contactref element="BUS" pad="A17"/>
<contactref element="U2" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="U4" pad="45"/>
</signal>
<signal name="A14">
<contactref element="BUS" pad="A16"/>
<contactref element="U2" pad="3"/>
<contactref element="U1" pad="3"/>
<contactref element="U4" pad="44"/>
</signal>
<signal name="A13">
<contactref element="BUS" pad="A15"/>
<contactref element="U2" pad="28"/>
<contactref element="U1" pad="28"/>
<contactref element="U3" pad="28"/>
<contactref element="U4" pad="4"/>
</signal>
<signal name="A10">
<contactref element="BUS" pad="A13"/>
<contactref element="U2" pad="23"/>
<contactref element="U1" pad="23"/>
<contactref element="U3" pad="23"/>
<contactref element="U4" pad="77"/>
</signal>
<signal name="A9">
<contactref element="BUS" pad="A12"/>
<contactref element="U2" pad="26"/>
<contactref element="U1" pad="26"/>
<contactref element="U3" pad="26"/>
<contactref element="U4" pad="84"/>
</signal>
<signal name="A7">
<contactref element="BUS" pad="A11"/>
<contactref element="U2" pad="5"/>
<contactref element="U1" pad="5"/>
<contactref element="U3" pad="5"/>
<contactref element="U4" pad="65"/>
</signal>
<signal name="A4">
<contactref element="BUS" pad="A9"/>
<contactref element="U2" pad="8"/>
<contactref element="U1" pad="8"/>
<contactref element="U3" pad="8"/>
<contactref element="U4" pad="68"/>
</signal>
<signal name="A3">
<contactref element="BUS" pad="A8"/>
<contactref element="U2" pad="9"/>
<contactref element="U1" pad="9"/>
<contactref element="U3" pad="9"/>
<contactref element="U4" pad="69"/>
</signal>
<signal name="A1">
<contactref element="BUS" pad="A7"/>
<contactref element="U2" pad="11"/>
<contactref element="U1" pad="11"/>
<contactref element="U3" pad="11"/>
<contactref element="U6" pad="12"/>
<contactref element="U4" pad="73"/>
</signal>
<signal name="D6">
<contactref element="BUS" pad="A5"/>
<contactref element="U3" pad="20"/>
<contactref element="U2" pad="20"/>
<contactref element="U1" pad="20"/>
<contactref element="U6" pad="8"/>
<contactref element="U4" pad="56"/>
<contactref element="U5" pad="10"/>
</signal>
<signal name="D5">
<contactref element="BUS" pad="A4"/>
<contactref element="U3" pad="19"/>
<contactref element="U2" pad="19"/>
<contactref element="U1" pad="19"/>
<contactref element="U4" pad="52"/>
<contactref element="U6" pad="5"/>
<contactref element="U5" pad="9"/>
</signal>
<signal name="D3">
<contactref element="BUS" pad="A3"/>
<contactref element="U3" pad="17"/>
<contactref element="U2" pad="17"/>
<contactref element="U1" pad="17"/>
<contactref element="U6" pad="4"/>
<contactref element="U4" pad="55"/>
<contactref element="U5" pad="7"/>
</signal>
<signal name="D0">
<contactref element="BUS" pad="A1"/>
<contactref element="U3" pad="13"/>
<contactref element="U2" pad="13"/>
<contactref element="U1" pad="13"/>
<contactref element="U6" pad="14"/>
<contactref element="U4" pad="48"/>
<contactref element="U5" pad="4"/>
</signal>
<signal name="+5V">
<contactref element="U2" pad="32"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="32"/>
<contactref element="U4" pad="38"/>
<contactref element="U4" pad="26"/>
<contactref element="U4" pad="13"/>
<contactref element="U4" pad="3"/>
<contactref element="U4" pad="78"/>
<contactref element="U4" pad="66"/>
<contactref element="U4" pad="43"/>
<contactref element="U4" pad="53"/>
<contactref element="C3" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="U3" pad="32"/>
<contactref element="C8" pad="1"/>
<contactref element="U6" pad="23"/>
<contactref element="U6" pad="35"/>
<contactref element="U6" pad="15"/>
<contactref element="U6" pad="3"/>
<contactref element="C5" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="BUS" pad="A26"/>
<contactref element="J3" pad="4"/>
<contactref element="J4" pad="4"/>
<contactref element="RN1" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="AUX" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="U5" pad="24"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="!IDE_IOW">
<contactref element="J2" pad="23"/>
<contactref element="U4" pad="31"/>
</signal>
<signal name="!IDE_IOR">
<contactref element="J2" pad="25"/>
<contactref element="U4" pad="30"/>
</signal>
<signal name="IDE_A1">
<contactref element="J2" pad="33"/>
<contactref element="U4" pad="34"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="IDE_A0">
<contactref element="J2" pad="35"/>
<contactref element="U4" pad="36"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="!IDE_CS0">
<contactref element="J2" pad="37"/>
<contactref element="U4" pad="35"/>
</signal>
<signal name="IDE_D8">
<contactref element="J2" pad="4"/>
<contactref element="U4" pad="9"/>
</signal>
<signal name="IDE_D9">
<contactref element="J2" pad="6"/>
<contactref element="U4" pad="10"/>
</signal>
<signal name="IDE_D10">
<contactref element="J2" pad="8"/>
<contactref element="U4" pad="16"/>
</signal>
<signal name="IDE_D11">
<contactref element="J2" pad="10"/>
<contactref element="U4" pad="18"/>
</signal>
<signal name="IDE_D12">
<contactref element="J2" pad="12"/>
<contactref element="U4" pad="20"/>
</signal>
<signal name="IDE_D13">
<contactref element="J2" pad="14"/>
<contactref element="U4" pad="25"/>
</signal>
<signal name="IDE_D14">
<contactref element="J2" pad="16"/>
<contactref element="U4" pad="27"/>
</signal>
<signal name="IDE_D15">
<contactref element="J2" pad="18"/>
<contactref element="U4" pad="28"/>
</signal>
<signal name="IDE_A2">
<contactref element="J2" pad="36"/>
<contactref element="U4" pad="33"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="!CS_ROM">
<contactref element="U3" pad="22"/>
<contactref element="U4" pad="41"/>
</signal>
<signal name="IDE_D7">
<contactref element="J2" pad="3"/>
<contactref element="U4" pad="11"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="IDE_D6">
<contactref element="J2" pad="5"/>
<contactref element="U4" pad="12"/>
</signal>
<signal name="IDE_D5">
<contactref element="J2" pad="7"/>
<contactref element="U4" pad="15"/>
</signal>
<signal name="IDE_D4">
<contactref element="J2" pad="9"/>
<contactref element="U4" pad="17"/>
</signal>
<signal name="IDE_D3">
<contactref element="J2" pad="11"/>
<contactref element="U4" pad="21"/>
</signal>
<signal name="IDE_D2">
<contactref element="J2" pad="13"/>
<contactref element="U4" pad="22"/>
</signal>
<signal name="IDE_D1">
<contactref element="J2" pad="15"/>
<contactref element="U4" pad="24"/>
</signal>
<signal name="IDE_D0">
<contactref element="J2" pad="17"/>
<contactref element="U4" pad="29"/>
</signal>
<signal name="IRQ7">
<contactref element="BUS" pad="B29"/>
<contactref element="SW1" pad="12"/>
</signal>
<signal name="IRQ2">
<contactref element="BUS" pad="A29"/>
<contactref element="SW1" pad="11"/>
</signal>
<signal name="IRQ1">
<contactref element="BUS" pad="A28"/>
<contactref element="SW1" pad="10"/>
</signal>
<signal name="!RESET">
<contactref element="U6" pad="26"/>
<contactref element="J2" pad="1"/>
<contactref element="U5" pad="18"/>
</signal>
<signal name="CFG2">
<contactref element="SW1" pad="8"/>
<contactref element="U4" pad="6"/>
<contactref element="RN1" pad="3"/>
</signal>
<signal name="CLK">
<contactref element="BUS" pad="A24"/>
<contactref element="U4" pad="83"/>
<contactref element="U6" pad="43"/>
</signal>
<signal name="!RTC_CS">
<contactref element="U6" pad="21"/>
<contactref element="U5" pad="13"/>
</signal>
<signal name="!CS_RAM0">
<contactref element="U2" pad="22"/>
<contactref element="U4" pad="58"/>
</signal>
<signal name="!CS_RAM1">
<contactref element="U1" pad="22"/>
<contactref element="U4" pad="76"/>
</signal>
<signal name="CFG3">
<contactref element="SW1" pad="7"/>
<contactref element="U4" pad="8"/>
<contactref element="RN1" pad="2"/>
</signal>
<signal name="!IDE_CS1">
<contactref element="J2" pad="38"/>
<contactref element="U4" pad="37"/>
</signal>
<signal name="PDEC">
<contactref element="U6" pad="18"/>
<contactref element="U4" pad="51"/>
</signal>
<signal name="RTC_ALE">
<contactref element="U6" pad="20"/>
<contactref element="U5" pad="14"/>
</signal>
<signal name="!IOW">
<contactref element="BUS" pad="A21"/>
<contactref element="U6" pad="2"/>
</signal>
<signal name="CFG1">
<contactref element="SW1" pad="9"/>
<contactref element="U4" pad="5"/>
<contactref element="RN1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="POST" pad="3"/>
<contactref element="RA1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="POST" pad="8"/>
<contactref element="RA1" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="POST" pad="10"/>
<contactref element="RA1" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="POST" pad="7"/>
<contactref element="RA1" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="POST" pad="6"/>
<contactref element="RA1" pad="7"/>
</signal>
<signal name="N$12">
<contactref element="POST" pad="1"/>
<contactref element="RA1" pad="6"/>
</signal>
<signal name="!DASP">
<contactref element="HDLED" pad="K"/>
<contactref element="J5" pad="1"/>
<contactref element="J2" pad="39"/>
</signal>
<signal name="S_TCK">
<contactref element="U6" pad="32"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="S_TDO">
<contactref element="U6" pad="38"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="POST" pad="2"/>
<contactref element="RA1" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="POST" pad="5"/>
<contactref element="RA1" pad="8"/>
</signal>
<signal name="LED_C">
<contactref element="U6" pad="37"/>
<contactref element="RA1" pad="11"/>
</signal>
<signal name="LED_F">
<contactref element="U6" pad="39"/>
<contactref element="RA1" pad="10"/>
</signal>
<signal name="LED_G">
<contactref element="U6" pad="29"/>
<contactref element="RA1" pad="16"/>
</signal>
<signal name="LED_A">
<contactref element="U6" pad="34"/>
<contactref element="RA1" pad="14"/>
</signal>
<signal name="LED_B">
<contactref element="U6" pad="31"/>
<contactref element="RA1" pad="15"/>
</signal>
<signal name="LED_E">
<contactref element="U6" pad="33"/>
<contactref element="RA1" pad="13"/>
</signal>
<signal name="LED_DP">
<contactref element="U6" pad="36"/>
<contactref element="RA1" pad="12"/>
</signal>
<signal name="LED_D">
<contactref element="U6" pad="40"/>
<contactref element="RA1" pad="9"/>
</signal>
<signal name="LED_C1">
<contactref element="U6" pad="28"/>
<contactref element="POST" pad="9"/>
</signal>
<signal name="LED_C2">
<contactref element="U6" pad="27"/>
<contactref element="POST" pad="4"/>
</signal>
<signal name="S_TMS">
<contactref element="U6" pad="13"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="S_TDI">
<contactref element="U6" pad="7"/>
<contactref element="J4" pad="9"/>
</signal>
<signal name="M_TCK">
<contactref element="U4" pad="62"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="M_TMS">
<contactref element="U4" pad="23"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="M_TDI">
<contactref element="U4" pad="14"/>
<contactref element="J3" pad="9"/>
</signal>
<signal name="M_TDO">
<contactref element="U4" pad="71"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="!RTC_OE">
<contactref element="U6" pad="25"/>
<contactref element="U5" pad="17"/>
</signal>
<signal name="!RTC_WE">
<contactref element="U6" pad="24"/>
<contactref element="U5" pad="15"/>
</signal>
<signal name="!RTC_IRQ">
<contactref element="SW1" pad="1"/>
<contactref element="SW1" pad="2"/>
<contactref element="SW1" pad="3"/>
<contactref element="U5" pad="19"/>
</signal>
<signal name="!IOR">
<contactref element="BUS" pad="A20"/>
<contactref element="U6" pad="44"/>
</signal>
<signal name="N$1">
<contactref element="HDLED" pad="A"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="BUS" pad="A10"/>
<contactref element="BUS" pad="B4"/>
<contactref element="BUS" pad="B8"/>
<contactref element="BUS" pad="B15"/>
<contactref element="BUS" pad="B17"/>
<contactref element="BUS" pad="A22"/>
<contactref element="BUS" pad="A18"/>
<contactref element="BUS" pad="B28"/>
<contactref element="BUS" pad="B20"/>
<contactref element="BUS" pad="B24"/>
<contactref element="U2" pad="16"/>
<contactref element="U1" pad="16"/>
<contactref element="U4" pad="72"/>
<contactref element="U4" pad="7"/>
<contactref element="U4" pad="19"/>
<contactref element="U4" pad="82"/>
<contactref element="U4" pad="59"/>
<contactref element="U4" pad="47"/>
<contactref element="U4" pad="32"/>
<contactref element="U4" pad="42"/>
<contactref element="U3" pad="16"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="U6" pad="42"/>
<contactref element="U6" pad="10"/>
<contactref element="U6" pad="22"/>
<contactref element="U6" pad="30"/>
<contactref element="C5" pad="2"/>
<contactref element="U6" pad="41"/>
<contactref element="C4" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="J2" pad="19"/>
<contactref element="J2" pad="30"/>
<contactref element="J2" pad="28"/>
<contactref element="J2" pad="26"/>
<contactref element="J2" pad="24"/>
<contactref element="J2" pad="22"/>
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="J3" pad="10"/>
<contactref element="J4" pad="10"/>
<contactref element="J4" pad="2"/>
<contactref element="SW1" pad="4"/>
<contactref element="SW1" pad="5"/>
<contactref element="SW1" pad="6"/>
<contactref element="R3" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="AUX" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="U5" pad="12"/>
<contactref element="U5" pad="16"/>
<contactref element="VBAT" pad="-"/>
<contactref element="BAT" pad="2"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="ROM_A17">
<contactref element="U3" pad="30"/>
<contactref element="U4" pad="40"/>
</signal>
<signal name="ROM_A14">
<contactref element="U3" pad="29"/>
<contactref element="U4" pad="39"/>
</signal>
<signal name="N$6">
<contactref element="J5" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="J2" pad="20"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="+VBAT">
<contactref element="U5" pad="20"/>
<contactref element="VBAT" pad="+"/>
<contactref element="BAT" pad="1"/>
</signal>
<signal name="X1">
<contactref element="U5" pad="2"/>
</signal>
<signal name="X2">
<contactref element="U5" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
