<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>ON</text>
<text>ON</text>
<text>ON</text>
<text>ON</text>
<text>ON</text>
<text>ON</text>
<text>ON</text>
<text>ON</text>
<text>ON</text>
<text>ON</text>
<text>ON</text>
<text>ON</text>
<text>ON</text>
<text>ON</text>
<text>ON</text>
<text>OFF</text>
<text>OFF</text>
<text>OFF</text>
<text>OFF</text>
<text>OFF</text>
<text>OFF</text>
<text>OFF</text>
<text>OFF</text>
<text>OFF</text>
<text>OFF</text>
<text>OFF</text>
<text>OFF</text>
<text>200h</text>
<text>240h</text>
<text>280h</text>
<text>2C0h</text>
<text>300h</text>
<text>340h</text>
<text>380h</text>
<text>3C0h</text>
<text>SW4</text>
<text>SW5</text>
<text>SW6</text>
<text>ADDR</text>
<text>OFF</text>
<text>OFF</text>
<text>OFF</text>
<text>OFF</text>
<text>OFF</text>
<text>OFF</text>
<text>SW1</text>
<text>SW2</text>
<text>SW3</text>
<text>IRQ</text>
<text>IRQ2</text>
<text>IRQ3</text>
<text>IRQ4</text>
<text>NE2000 Tandy PLUS Ethernet</text>
<wire x1="46.99" y1="-138.43" x2="46.99" y2="-237.49" width="0" layer="20"/>
<text>Rev.P2</text>
</plain>
<libraries>
<library name="alan_common">
<description>Alan's frequently used manually inputted parts</description>
<packages>
<package name="TANDY_PCPLUS_SLAVE">
</package>
<package name="TQFP64_7MM">
</package>
<package name="SMT_0402">
</package>
<package name="NXP_TSSOP20_65">
</package>
<package name="SW_DIP-6_ROUND">
</package>
<package name="SOT23-6">
</package>
<package name="TP_ROUND_LARGE">
</package>
<package name="ABRACON_ASDMB">
</package>
<package name="RN_SIP4">
</package>
<package name="MICROCHIP_SOIC-8SN">
</package>
<package name="SMT_0805">
</package>
<package name="RJ45_WIZNET">
</package>
<package name="SMT_0603">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PLUS_" library="alan_common" package="TANDY_PCPLUS_SLAVE" value="TANDY_PLUS_SLAVE2"/>
<element name="U1" library="alan_common" package="TQFP64_7MM" value="AX88796B"/>
<element name="R1" library="alan_common" package="SMT_0402" value="4.7K/DNI">
<attribute name="REELCODE" value="R"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="U$2" library="alan_common" package="NXP_TSSOP20_65" value="16V8_T"/>
<element name="SW1" library="alan_common" package="SW_DIP-6_ROUND" value="SW_DIP-6R"/>
<element name="U2" library="alan_common" package="SOT23-6" value="93C46"/>
<element name="WAKE" library="alan_common" package="TP_ROUND_LARGE" value="TEST_POINT_LARGE">
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".1"/>
</element>
<element name="R2" library="alan_common" package="SMT_0402" value="12.1K">
<attribute name="REELCODE" value="R"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C1" library="alan_common" package="SMT_0402" value=".1uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="XO1" library="alan_common" package="ABRACON_ASDMB" value="25 MHz"/>
<element name="R3" library="alan_common" package="SMT_0402" value="22">
<attribute name="REELCODE" value="R"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C2" library="alan_common" package="SMT_0402" value=".1uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C3" library="alan_common" package="SMT_0402" value="2.2uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C4" library="alan_common" package="SMT_0402" value=".1uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C5" library="alan_common" package="SMT_0402" value="2.2uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C6" library="alan_common" package="SMT_0402" value=".1uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C7" library="alan_common" package="SMT_0402" value="2.2uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C8" library="alan_common" package="SMT_0402" value=".1uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C9" library="alan_common" package="SMT_0402" value="2.2uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C10" library="alan_common" package="SMT_0402" value=".1uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C11" library="alan_common" package="SMT_0402" value="2.2uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C12" library="alan_common" package="SMT_0402" value=".1uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="FB1" library="alan_common" package="SMT_0402" value="600@100Mhz">
<attribute name="REELCODE" value="FB"/>
<attribute name="NAME"/>
</element>
<element name="FB2" library="alan_common" package="SMT_0402" value="600@100Mhz">
<attribute name="REELCODE" value="FB"/>
<attribute name="NAME"/>
</element>
<element name="FB3" library="alan_common" package="SMT_0402" value="600@100Mhz">
<attribute name="REELCODE" value="FB"/>
<attribute name="NAME"/>
</element>
<element name="FB4" library="alan_common" package="SMT_0402" value="600@100Mhz">
<attribute name="REELCODE" value="FB"/>
<attribute name="NAME"/>
</element>
<element name="FB5" library="alan_common" package="SMT_0402" value="600@100Mhz">
<attribute name="REELCODE" value="FB"/>
<attribute name="NAME"/>
</element>
<element name="C13" library="alan_common" package="SMT_0402" value=".1uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C14" library="alan_common" package="SMT_0402" value="2.2uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C15" library="alan_common" package="SMT_0402" value=".1uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C16" library="alan_common" package="SMT_0402" value=".1uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C17" library="alan_common" package="SMT_0402" value="2.2uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C18" library="alan_common" package="SMT_0402" value="2.2uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="RN1" library="alan_common" package="RN_SIP4" value="10K"/>
<element name="U3" library="alan_common" package="MICROCHIP_SOIC-8SN" value="REG_LDO_SO">
<attribute name="HEIGHT" value="1.8"/>
</element>
<element name="C19" library="alan_common" package="SMT_0805" value="4.7uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value="1"/>
</element>
<element name="C20" library="alan_common" package="SMT_0805" value="4.7uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value="1"/>
</element>
<element name="J1" library="alan_common" package="RJ45_WIZNET" value="RB1-125BAG1A"/>
<element name="R4" library="alan_common" package="SMT_0402" value="330">
<attribute name="REELCODE" value="R"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="R5" library="alan_common" package="SMT_0402" value="330">
<attribute name="REELCODE" value="R"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="R6" library="alan_common" package="SMT_0402" value="50">
<attribute name="REELCODE" value="R"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="R7" library="alan_common" package="SMT_0402" value="50">
<attribute name="REELCODE" value="R"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="R8" library="alan_common" package="SMT_0402" value="50">
<attribute name="REELCODE" value="R"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="R9" library="alan_common" package="SMT_0402" value="50">
<attribute name="REELCODE" value="R"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C21" library="alan_common" package="SMT_0402" value=".1uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C22" library="alan_common" package="SMT_0402" value=".1uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C23" library="alan_common" package="SMT_0402" value=".1uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="C24" library="alan_common" package="SMT_0402" value="1uF">
<attribute name="REELCODE" value="C"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="R10" library="alan_common" package="SMT_0402" value="330">
<attribute name="REELCODE" value="R"/>
<attribute name="NAME"/>
<attribute name="HEIGHT" value=".35"/>
</element>
<element name="FULL" library="alan_common" package="SMT_0603" value="LED_0603">
<attribute name="NAME"/>
<attribute name="NAME"/>
<attribute name="REELCODE" value="LED"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="PLUS_" pad="B31"/>
<contactref element="PLUS_" pad="B10"/>
<contactref element="PLUS_" pad="B1"/>
<contactref element="R1" pad="1"/>
<contactref element="PLUS_" pad="GND2"/>
<contactref element="PLUS_" pad="GND1"/>
<contactref element="U1" pad="12"/>
<contactref element="U1" pad="63"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="13"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="11"/>
<contactref element="U1" pad="58"/>
<contactref element="U1" pad="26"/>
<contactref element="U1" pad="18"/>
<contactref element="R2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="XO1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U$2" pad="10"/>
<contactref element="C12" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="SW1" pad="6"/>
<contactref element="SW1" pad="5"/>
<contactref element="SW1" pad="4"/>
<contactref element="U$2" pad="8"/>
<contactref element="U$2" pad="11"/>
<contactref element="C19" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="U3" pad="1"/>
<contactref element="C22" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="C24" pad="2"/>
<contactref element="J1" pad="S2"/>
<contactref element="J1" pad="S1"/>
</signal>
<signal name="+5V">
<contactref element="PLUS_" pad="B3"/>
<contactref element="U$2" pad="20"/>
<contactref element="RN1" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="+12V">
</signal>
<signal name="-12V">
</signal>
<signal name="SD0">
<contactref element="U1" pad="42"/>
<contactref element="PLUS_" pad="A9"/>
</signal>
<signal name="SD1">
<contactref element="U1" pad="41"/>
<contactref element="PLUS_" pad="A8"/>
</signal>
<signal name="SD2">
<contactref element="U1" pad="40"/>
<contactref element="PLUS_" pad="A7"/>
</signal>
<signal name="SD3">
<contactref element="U1" pad="39"/>
<contactref element="PLUS_" pad="A6"/>
</signal>
<signal name="SD4">
<contactref element="U1" pad="38"/>
<contactref element="PLUS_" pad="A5"/>
</signal>
<signal name="SD5">
<contactref element="U1" pad="37"/>
<contactref element="PLUS_" pad="A4"/>
</signal>
<signal name="SD6">
<contactref element="U1" pad="36"/>
<contactref element="PLUS_" pad="A3"/>
</signal>
<signal name="SD7">
<contactref element="U1" pad="35"/>
<contactref element="PLUS_" pad="A2"/>
</signal>
<signal name="AEN">
<contactref element="PLUS_" pad="A11"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="51"/>
</signal>
<signal name="SA5">
<contactref element="U1" pad="45"/>
<contactref element="PLUS_" pad="A26"/>
</signal>
<signal name="SA4">
<contactref element="U1" pad="46"/>
<contactref element="PLUS_" pad="A27"/>
</signal>
<signal name="SA3">
<contactref element="U1" pad="47"/>
<contactref element="PLUS_" pad="A28"/>
</signal>
<signal name="SA2">
<contactref element="U1" pad="48"/>
<contactref element="PLUS_" pad="A29"/>
</signal>
<signal name="SA1">
<contactref element="U1" pad="49"/>
<contactref element="PLUS_" pad="A30"/>
</signal>
<signal name="SA0">
<contactref element="U1" pad="50"/>
<contactref element="PLUS_" pad="A31"/>
</signal>
<signal name="IRQ4">
<contactref element="PLUS_" pad="B24"/>
<contactref element="SW1" pad="3"/>
</signal>
<signal name="IRQ3">
<contactref element="PLUS_" pad="B25"/>
<contactref element="SW1" pad="2"/>
</signal>
<signal name="IRQ2">
<contactref element="PLUS_" pad="B4"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="PLUS_" pad="B2"/>
<contactref element="U$2" pad="9"/>
</signal>
<signal name="!IOWR">
<contactref element="PLUS_" pad="B13"/>
<contactref element="U1" pad="54"/>
</signal>
<signal name="!IORD">
<contactref element="PLUS_" pad="B14"/>
<contactref element="U1" pad="53"/>
</signal>
<signal name="!CS">
<contactref element="U1" pad="52"/>
<contactref element="U$2" pad="13"/>
</signal>
<signal name="IRQ">
<contactref element="U1" pad="23"/>
<contactref element="SW1" pad="12"/>
<contactref element="SW1" pad="11"/>
<contactref element="SW1" pad="10"/>
</signal>
<signal name="N$5">
<contactref element="WAKE" pad="1"/>
<contactref element="U1" pad="22"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="64"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="!RESET">
<contactref element="U1" pad="17"/>
<contactref element="U$2" pad="12"/>
</signal>
<signal name="+3V3">
<contactref element="C1" pad="1"/>
<contactref element="U2" pad="6"/>
<contactref element="C2" pad="1"/>
<contactref element="XO1" pad="4"/>
<contactref element="FB3" pad="2"/>
<contactref element="FB5" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="FB4" pad="2"/>
<contactref element="C20" pad="1"/>
<contactref element="U3" pad="3"/>
<contactref element="U3" pad="7"/>
<contactref element="U3" pad="6"/>
<contactref element="U3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="FULL" pad="1"/>
</signal>
<signal name="EECS">
<contactref element="U2" pad="5"/>
<contactref element="U1" pad="21"/>
</signal>
<signal name="EECLK">
<contactref element="U2" pad="4"/>
<contactref element="U1" pad="20"/>
</signal>
<signal name="EEDIO">
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="1"/>
<contactref element="U1" pad="19"/>
</signal>
<signal name="N$1">
<contactref element="XO1" pad="3"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R3" pad="2"/>
<contactref element="U1" pad="61"/>
</signal>
<signal name="SA6">
<contactref element="PLUS_" pad="A25"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="SA9">
<contactref element="PLUS_" pad="A22"/>
<contactref element="U$2" pad="7"/>
</signal>
<signal name="SA8">
<contactref element="PLUS_" pad="A23"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="SA7">
<contactref element="PLUS_" pad="A24"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="VDD3IO">
<contactref element="U1" pad="44"/>
<contactref element="U1" pad="25"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="FB5" pad="1"/>
</signal>
<signal name="VCC3R3">
<contactref element="U1" pad="10"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="FB4" pad="1"/>
</signal>
<signal name="VCC3A3">
<contactref element="U1" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="FB3" pad="1"/>
<contactref element="J1" pad="R3"/>
<contactref element="C24" pad="1"/>
<contactref element="C23" pad="1"/>
</signal>
<signal name="VCCK">
<contactref element="U1" pad="24"/>
<contactref element="U1" pad="43"/>
<contactref element="U1" pad="59"/>
<contactref element="C12" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="FB1" pad="1"/>
</signal>
<signal name="VCC18A">
<contactref element="U1" pad="60"/>
<contactref element="U1" pad="5"/>
<contactref element="C10" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="FB2" pad="1"/>
</signal>
<signal name="LED_COL">
<contactref element="U1" pad="16"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="LED_ACT">
<contactref element="U1" pad="14"/>
<contactref element="J1" pad="L4"/>
</signal>
<signal name="LED_SPD">
<contactref element="U1" pad="15"/>
<contactref element="J1" pad="L2"/>
</signal>
<signal name="TPO-">
<contactref element="U1" pad="7"/>
<contactref element="J1" pad="R2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="TPO+">
<contactref element="U1" pad="6"/>
<contactref element="J1" pad="R1"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="TPI-">
<contactref element="U1" pad="4"/>
<contactref element="J1" pad="R8"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="TPI+">
<contactref element="U1" pad="3"/>
<contactref element="J1" pad="R7"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="+1V8">
<contactref element="U1" pad="9"/>
<contactref element="FB1" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="FB2" pad="2"/>
</signal>
<signal name="SEL2">
<contactref element="SW1" pad="7"/>
<contactref element="RN1" pad="2"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="SEL1">
<contactref element="SW1" pad="8"/>
<contactref element="RN1" pad="3"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="SEL0">
<contactref element="SW1" pad="9"/>
<contactref element="RN1" pad="4"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R4" pad="1"/>
<contactref element="J1" pad="L1"/>
</signal>
<signal name="N$7">
<contactref element="R5" pad="1"/>
<contactref element="J1" pad="L3"/>
</signal>
<signal name="N$3">
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="C21" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="C22" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="FULL" pad="2"/>
<contactref element="R10" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
